| SONATA(YF) >2013 > G 2.4 GDI > Emission Control System > Evaporative Emission Control System > Canister>Repair procedures |

Removal

1. | Disconnect the canister close valve connector (A).

2. | Disconnect the ventilation tube quick-connector (B) and the vapor tube quick-connectors (C, D).

3. | Remove the installation bolts (E), and then remove the canister.

Inspection

1. | Check for the following items visually. - Cracks or leakage of the canister - Loose connection, distortion, or damage of the vapor hose/tube A: Canister ↔ Atmosphere B: Canister ↔ Fuel Tank
C: Canister ↔ Intake Manifold

Installation

Installation is the reverse of removal.

Canister installation bolt:
3.9 ~ 5.9 N.m (0.4 ~ 0.6 kgf.m, 2.9 ~ 4.3 lb-ft)