| SONATA(YF) >2012 > G 2.4 GDI > Suspension System > Rear Suspension System > Rear Stabilizer Bar>Repair procedures |

Replacement

1. | Remove the rear wheel & tire.

Tightening torque:
88.3 ~ 107.9 N.m (9.0 ~ 11.0 kgf.m, 65.1 ~ 79.6 lb-ft)

Be careful not to damage to the hub bolts when removing the rear wheel & tire.

2. | Loosen the nut and then remove the rear stabilizer link (B) with the rear lower arm (A).

Tightening torque:
98.1 ~ 117.7 N.m (10.0 ~ 12.0 kgf.m, 72.3 ~ 86.8 lb-ft)

3. | Loosen the nut and then remove the stabilizer link (A) with the rear stabilizer bar.

Tightening torque:
98.1 ~ 117.7 N.m (10.0 ~ 12.0 kgf.m, 72.3 ~ 86.8 lb-ft)

4. | Loosen the mounting bolt and then remove the stabilizer bar (B) with the sub frame (A).

Tightening torque:
44.1 ~ 53.9 N.m (4.5 ~ 5.5 kgf.m, 32.5 ~ 39.8 lb-ft)

5. | Installation is the reverse of removal.

Inspection

1. | Check the rear stabilizer bar for deformation.

2. | Check the rear stabilizer link ball joint for damage.