| SONATA(YF) >2012 > G 2.4 GDI > Body (Interior and Exterior) > Body Dimensions>General Information |

General

1. | Basically, all measurements in this manual are taken with a tracking gauge.

2. | When a measuring tape is used, check to be sure there is no elongation, twisting or bending.

3. | For measuring dimensions, both projected dimension and actual-measurement dimension are used in this manual.

Measurement Method

Projected Dimensions

1. | These are the dimensions measured when the measurement points are projected into the reference plane, and are the reference dimensions used for body alterations.

2. | If the length of the tracking gauge probes is adjustable, make the measurement by lengthening one probe by the amount equivalent to the difference in height of the two surfaces.

Actual-Measurement Dimensions

1. | These dimensions indicate the actual linear distance between measurement points, and are the reference dimensions for use if a tracking gauge is used for measurement.

2. | Measure by first adjusting both probes to the same length (A=A').

Check the probes and gauge itself to make sure there is no free play.

Measurement Point

1. | Measurements should be taken at the hole center.