| SONATA(YF) >2012 > G 2.4 GDI > Body Electrical System > Lighting System > Room Lamp>Repair procedures |

Inspection

Room Lamp

1. | Check that the switch operates properly after disconnecting the room lamp connector (A).

Removal

Room Lamp

1. | Disconnect the negative(-) battery terminal.

2. | Carefully remove the lens (A) using a small screwdriver.

3. | Remove the bulb.

4. | Remove the room lamp after loosening the mounting screws.

5. | Remove the room lamp assembly (A) from the head lining after disconnecting the connector.

Vanity Lamp

1. | Disconnect the negative (-) battery terminal.

2. | Remove the vanity lamp (A) prying out with a small screwdriver.

3. | Remove the vanity lamp assembly after disconnecting the connector (A).

Installation

Room Lamp

1. | Reconnect the connector.

2. | Install the room lamp assembly.

3. | Install the len.

Vanity Lamp

1. | Reconnect the vanity lamp connector.

2. | Install the vanity lamp.