| SONATA(YF) >2012 > G 2.4 GDI > Body Electrical System > Audio > Audio Unit>Components and Components Location |

Components

Terminal specification (PA710S)

Pin NO | Comments | Remarks | Output voltage (V)
A1 | Loudspeaker Rear Left + | Needed connection to the car | ANALOG output
A2 | Loudspeaker Front Left + | Needed connection to the car | ANALOG output
A3 | Loudspeaker Front Right + | Needed connection to the car | ANALOG output
A4 | Loudspeaker Rear Right + | Needed connection to the car | ANALOG output
A7 | Ignition status checking for reliable phone connection | (optional for Hands Free Kit) | -
A8 | Rheostat from vehicle + | Needed connection to the car | -
A9 | Illumination DIM cancel spec. | Needed connection to the car | -
A10 | Loudspeaker Rear Left - | Needed connection to the car | ANALOG output
A11 | Loudspeaker Front Left - | Needed connection to the car | ANALOG output
A12 | Loudspeaker Front Right - | Needed connection to the car | ANALOG output
A13 | Loudspeaker Rear Right - | Needed connection to the car | ANALOG output
A17 | Rheostat from vehicle - | Needed connection to the car | -
A18 | Remote supply for motorised antenna | Needed connection to the car | 9 to 18
B4 | Steel wheel remote control input | Needed connection to the car |
B6 | USB data line | (optional for USB Control) | 3.2 to 3.45
B7 | USB/iPod power (5V, MAX 1.1A) | (optional for USB Control) | 4.9 to 5.1
B8 | AUX ST sound R-CH input | Needed connection to the car | -
B9 | AUX ST sound GND | Needed connection to the car | -
B10 | Bluetooth H/F voice input | (optional for B/T hands free) | -
B11 | ACC | Needed connection to the car | -
B12 | Fused battery power supply (10A) | Needed connection to the car | -
B16 | Speed signal from vehicle | Needed connection to the car | -
B17 | Remote control GND | Needed connection to the car | GND
B18 | USB data line | (optional for USB Control) | 3.2 to 3.45
B19 | i Pod detection line | (optional for USB Control) | GND
B20 | AUX connection detect | Needed connection to the car | -
B21 | AUX ST sound L-CH input | Needed connection to the car | -
B22 | Bluetooth H/F voice input GND | (optional for B/T hands free) | -
B24 | Ground of Power Supply Line | Needed connection to the car | GND

Terminal specification (PA760S)

Pin NO | Comments | Remarks | Output voltage (V)
A5 | SPDIF digital signal GND | Needed connection to the car | GND
A6 | SPDIF digital signal negative | Needed connection to the car | 2 to 3.3
A7 | Ignition status checking for reliable phone connection | (optional for Hands Free Kit) | -
A8 | Rheostat from vehicle + | Needed connection to the car | -
A9 | Illumination DIM cancel spec. | Needed connection to the car | -
A15 | SPDIF digital signal positive | Needed connection to the car | 2 to 3.3
A17 | Rheostat from vehicle - | Needed connection to the car | -
A18 | Remote supply for motorised antenna | Needed connection to the car | 9 to 18
B1 | CAN-H I/F | Needed connection to the car | 3.6 to 5
B4 | Steel wheel remote control input | Needed connection to the car |
B6 | USB data line | (optional for USB Control) | 3.2 to 3.45
B7 | USB/iPod power (5V, MAX 1.1A) | (optional for USB Control) | 4.9 to 5.1
B8 | AUX ST sound R-CH input | Needed connection to the car | -
B9 | AUX ST sound GND | Needed connection to the car | -
B10 | Bluetooth H/F voice input | (optional for B/T hands free) | -
B11 | ACC | Needed connection to the car | -
B12 | Fused battery power supply (10A) | Needed connection to the car | -
B13 | CAN-L I/F | Needed connection to the car | 3.6 to 5.25
B16 | Speed signal from vehicle | Needed connection to the car | -
B17 | Remote control GND | Needed connection to the car | GND
B18 | USB data line | (optional for USB Control) | 3.2 to 3.45
B19 | i-Pod detection line | (optional for USB Control) | GND
B20 | AUX connection detect | Needed connection to the car | -
B21 | AUX ST sound L-CH input | Needed connection to the car | -
B22 | Bluetooth H/F voice input GND | (optional for B/T hands free) | -
B24 | Ground of Power Supply Line | Needed connection to the car | GND