| SONATA(YF) >2012 > G 2.4 GDI > Body Electrical System > Ignition Switch Assembly>Repair procedures |

Removal

1. | Disconnect the negative (-) battery terminal.

2. | Remove the driver crash pad lower panel. (Refer to the BD group - "Crash pad")

3. | Remove the steering column upper and lower shrouds. (Refer to the BD group - "Crash pad")

4. | Remove the wiper switch. (Refer to the BE group - "Multifunction switch")

5. | Remove the ignition switch after disconnecting the ignition switch 6P connector (A)

6. | Remove the key warning/immobilizer connector (A).

7. | After loosening the screw, remove the key warning switch and key Illumination (A).

8. | Pushing lock pin with key ACC.

9. | Remove the key lock cylinder (A).

Installation

1. | Install the key lock cylinder.

2. | Install the key warning switch and key Illumination.

3. | Install the key warning/immobilizer connector.

4. | Connect the ignition switch connector after Install the ignition switch.

5. | Install the wiper switch.

6. | Install the steering column shrouds.

7. | Install the driver crash pad lower panel.

Inspection

1. | Disconnect the ignition switch connector (A) and key warning switch connector (B) from the steering column.

2. | Check for continuity between the terminals.

3. | If continuity is not specified, replace the switch.