| SONATA(YF) >2013 > G 2.4 GDI > Body Electrical System > Smart key System > Smart key>Repair procedures |

Smart Key

Smart Key Code Saving

1. | Connect the DLC cable of GDS to the data link connector in driver side crash pad lower panel, turn the power on GDS.

2. | Select the vehicle model and then do "Smart key code saving".

3. | After selecting "Smart key teaching" menu, push "Enter" key, then the screen will be shown as below.

4. | After inserting the teaching key, push "ENTER" key.

5. | Input the "Pin code" for first key teaching.

6. | Confirm the message "First key teaching completed".

7. | Input the "Pin code" for second key teaching.

8. | Confirm the message "Second key teaching completed".

9. | Then the screen will be shown as below when key teaching process is completed.