| SONATA(YF) >2013 > G 2.4 GDI > Body (Interior and Exterior) > Bumper > Front Bumper>Repair procedures |

Replacement

• | Put on gloves to protect your hands.

• | When prying with a flat-tip screwdriver, wrap it with protective tape to prevent damage.

• | Take care not bend or scratch the cover and other parts.

1. | Remove the mounting clips.

2. | Remove the radiator upper cover mounting clips.

3. | After loosening the front bumper side’s mounting screw, then disconnect the side’s.

4. | Remove the front bumper after pull out the front bumper.

• | When you pull out the front bumper, the font bumper could be damaged by the projection (A).

5. | Disconnect the connector (A).

6. | Installation is the reverse of removal.