| SONATA(YF) >2012 > G 2.4 GDI > Body Electrical System > Windshield Wiper/Washer > Windshield Wiper-Washer Switch>Repair procedures |

Inspection

Check for continuity between the terminals while operating the wiper and washer switch. If it is not normal condition, replace wiper and wiper switch.

Wiper Switch

Washer Switch

Removal

1. | Remove the steering column upper and lower shrouds after removing 3 screws.

2. | Remove the wiper switch (A) by releasing the part.

3. | If necessary of removing the wiper & washer switch (A), release the lock of wiper switch using tool without removing the steering wheel and the clock spring.

Installation

1. | Install the wiper switch.

2. | Install the steering column upper and lower shrouds.