| SONATA(YF) >2012 > G 2.4 GDI > Body Electrical System > AVN System>Specifications |

Specifications

Item | Specification
Power source | DC 14.4V (-) ground
Frequency range / Channel space | FM : 87.9 ~ 107.9 MHz / 200 KHz AM : 530 ~ 1710 KHz / 10 KHz
Tuning type | PLL SYNTHESIZED TUNING
Impedance | 2 ohm x 4
Antenna | 80 pF 75 Ohm
Dark current | MAX 4mA (Head unit only)
S/N | FM : MIN 50 dB AM : MIN 40 dB
Temperature range | Operating : -20 °C~ +70 °C (-4 °F~ +158 °)F Storage : -30 °C~ +80 °C (-22 °F~ +316 °F)

GPS

Item | Specification
Frequency | 1.57542 GHz
Sensitivity level | - 144 dbm
Channel | 12CH

Speaker

Item | Specification
Input power (W or V) | Front | Max 50W
Rear | Max 50W
Midrange | Max 50W
Sub woofer | MAX 50W
Impedance (Ω) | Front | 2 ± 0.3
Rear | 2 ± 0.3
Midrange | 1.8 ± 0.3
Sub woofer | 2.5 ± 0.4
Number of speaker | 7