| SONATA(YF) >2013 > G 2.4 GDI > Restraint > Seat Belt Pretensioner > Anchor Pretensioner (APT)>Repair procedures |

Removal

1. | Disconnect the battery negative cable, and wait for at least three minutes before beginning work.

2. | Using a flat-trip screwdriver, remove the seat belt anchor pretensioner (A).

3. | Remove the door scuff trim. (Refer to the Body group- Interior trim)

4. | Remove the center pillar trim. (Refer to the Body group- Interior trim)

5. | Disconnect the anchor pretensioner connector.

6. | Loosen the anchor pretensioner mounting bolt and remove the anchor pretensioner.

Installation

1. | Remove ignition key from the vehicle.

2. | Disconnect the negative (-) cable from battery and wait for at least three minutes.

3. | Install the anchor pretensioner with a bolt.

Tightening torque :
39.2~53.9 N.m(4.0 ~ 5.5 kgf.m, 28.9 ~ 39.8 lb-ft)

4. | Connect the anchor pretensioner connector.

5. | Install the center pillar trim. (Refer to the Body group- Interior trim)

6. | Install the door scuff trim. (Refer to the Body group- Interior trim)

7. | Insert the seat belt to the anchor pretensioner (A).

Make sure the lock pin is connected in properly.

8. | Reconnect the battery negative cable.

9. | After installing the anchor pretensioner, confirm proper system operation:

A. | Turn the ignition switch ON; the SRS indicator light should be turned on for about six seconds and then go off.