| SONATA(YF) >2012 > G 2.4 GDI > Automatic Transaxle System > General Information>Specifications |

Specifications

Item | Specification
Transmission type | A6MF2
Engine model | Gasoline 2.4 GDI
Torque converter type | 3-element, 1-stage, 2-phase type
Torque converter size | Ø236 mm (9.2913 in.)
Oil pump system | Parachoid
Friction elements | Clutch: 2EA
Brake: 3EA
OWC : 1EA
Planetary gear | 3EA
Gear ratio | 1st | 4.212
2nd | 2.637
3rd | 1.8
4th | 1.386
5th | 1.000
6th | 0.772
Reverse | 3.385
Final gear ratio | 2.885
Fluid pressure balance piston | 2EA
Accumulator | 4EA
Solenoid valve | 8EA (VFS:6EA, ON/OFF:2EA)
Shift lever position | 4 Range (P,R,N,D)
Oil filter | 1EA

VFS: Variable Force Solenoid
Tightening Torques

Item | N.m | Kgf.m | lb-ft
TCM installation bolt | 9.8 ~ 11.8 | 1.0 ~ 1.2 | 7.2 ~ 8.7
Shift cable bracket mounting bolt | 14.7 ~ 21.6 | 1.5 ~ 2.2 | 10.9 ~ 15.9
Input shaft speed sensor mounting bolt | 9.8 ~ 11.8 | 1.0 ~ 1.2 | 7.2 ~ 8.7
Output shaft speed sensor mounting bolt | 9.8 ~ 11.8 | 1.0 ~ 1.2 | 7.2 ~ 8.7
Shift lever assembly bolt | 17.7 ~ 24.5 | 1.8 ~ 2.5 | 13.0 ~ 18.1
Inhibitor switch mounting bolt | 9.8 ~ 11.8 | 1.0 ~ 1.2 | 7.2 ~ 8.7
Valve body cover mounting bolt | 12.8 ~ 14.7 | 1.3 ~ 1.5 | 9.4 ~ 10.8
Eyebolt | 34.3 ~ 44.1 | 3.5 ~ 4.5 | 25.3 ~ 32.6
Oil drain plug | 34.3 ~ 44.1 | 3.5 ~ 4.5 | 25.3 ~ 32.6
Oil level plug | 34.3 ~ 44.1 | 3.5 ~ 4.5 | 25.3 ~ 32.6
Torque converter mounting bolt | 45.1 ~ 52.0 | 4.6 ~ 5.3 | 33.3 ~ 38.3
Automatic transaxle upper mounting bolt | 42.2 ~ 53.9 | 4.3 ~ 5.5 | 31.3 ~ 39.8
Automatic transaxle lower mounting bolt | 29.4 ~ 41.2 42.2 ~ 54.0 | 3.0 ~ 4.2 4.3 ~ 5.5 | 21.7 ~ 30.4 31.1 ~ 39.8
Automatic transaxle support bracket bolt | 68.6 ~ 93.2 | 7.0~ 9.5 | 50.6 ~ 68.7

Lubricants

Item | Specified lubricant | Quantity
Transaxle fluid | SK ATF SP-Ⅳ, MICHANG ATF SP-Ⅳ, NOCA ATF SP-Ⅳ, Hyundai Genuine ATF SP-Ⅳ | 7.1L (1.88 U.S gal., 7.50 U.S.qt., 6.24 Imp.qt.)

Sealant

Item | Specified sealant
Rear cover Torque converter housing Valve body cover | LOCTITE FMD-546 or THREE-BOND TB1281B