| SONATA(YF) >2012 > G 2.4 GDI > Body Electrical System > Fuel Filler Door > Fuel Filler Door Release Actuator>Repair procedures |

Inspection

1. | Remove the trunk room left side trim. (Refer to the BD group - "Interior trim")

2. | Open the fuel filler door and remove the housing (A).

Do not reuse the fuel filler door housing.

3. | Remove the fuel filler door release actuator (A) after loosening the mounting bolts.

4. | Disconnect the release actuator connector (A).

5. | Check for continuity between terminal No.1 and No.2. If there is no continuity, replace the fuel filler door opener.