| SONATA(YF) >2013 > G 2.4 GDI > Body Electrical System > Power Windows > Power Window Relay>Repair procedures |

Inspection

1. | Disconnect the negative (-) battery terminal.

2. | Remove the junction box.

3. | Check for continuity between the terminals.

4. | There should be continuity between the No.1 in the I/P-C and No.26(or 39) terminal in the I/P-A when power and ground are connected to the No.1 terminal in the I/P-C and ground.

5. | There should be no continuity between the No.1 terminal in the I/P-C and No.26(or 39) terminal in the I/P-A when power is disconnected. [Front] [Rear]