| SONATA(YF) >2012 > G 2.4 GDI > Body Electrical System > Fuel Filler Door > Fuel Filler Door Open Switch>Repair procedures |

Inspection

1. | Remove the switch assembly (A) from the crash pad lower panel.

2. | Disconnect the switch connector.

3. | Check for continuity between the terminal No.3 and No.4. If there is no continuity, replace the fuel filler door open switch. (1. Trunk B+, 2. Trunk solenoid, 3. Fuel filler B+ 4. Fuel filler door open solenoid)