| SONATA(YF) >2013 > G 2.4 GDI > Engine Mechanical System > Lubrication System > Oil Cooler>Repair procedures |

Removal

1. | Loosen the drain plug, and drain the coolant. Remove the radiator cap to speed draining.

2. | Disconnect the oil cooler coolant hoses (A).

3. | Remove the oil filter (A).

4. | Loosen the mounting bolt (A) and remove the oil cooler assembly (B).

Installation

1. | Apply a light coat of engine oil to the oil cooler packing surface (A), and then install the oil cooler with fix bolt (B).

Tightening torque:
44.1 ~ 53.9 N.m (4.5 ~ 5.5 kgf.m, 32.5 ~ 39.8 lb-ft)

Fix position of oil cooler stopper (A) where oil cooler resists on ladder frame stopper (B).

2. | Apply a light coat of engine oil to the oil filter packing surface (A), and then install the oil filter.

Tightening torque:
11.8 ~ 15.7 N.m (1.2 ~ 1.6 kgf.m, 8.7 ~ 11.6 lb-ft)

3. | Connect the oil cooler coolant hoses (B).

4. | Fill the radiator with coolant and check for leaks.