| SONATA(YF) >2013 > G 2.4 GDI > Body Electrical System > Seat Electrical > Power Seat Motor>Repair procedures |

Inspection

Power Seat Motor

1. | Disconnect the connectors for each motor. A : Front height motor B : Slide motor C : Rear height motor D : Recline motor
E : Lumber support motor

2. | With the battery connected directly to the motor terminals, check if the motors run smoothly.

3. | Reverse the connections and check that the motor rotates in reverse.

4. | If there is an abnormality, replace the motors.