| SONATA(YF) >2013 > G 2.4 GDI > Suspension System > Tire Pressure Monitoring System > TPMS Sensor>Repair procedures |

Removal

Handle the sensor with care.

1. | Remove the tire. (Refer to "Tire Removal")

2. | Remove the valve nut.

The valve nut should not be re-used.

3. | Discard the valve assembly.

Installation

Sensor Fit

• | Handle the sensor with care.

• | Avoid lubricant contact.

• | Ensure that the wheel to be fitted is designed for sensor mount. There should normally be a mark to indicate this.

• | Ensure that the valve hole and mating face of the wheel are clean.

1. | Slide the sensor-valve unit through the valve hole of the rim. Hold the sensor against the rim and the rubber grommet against the sealing surface.

2. | Insert the nut over the valve stem and then tighten the nut.

3. | Continue to tightening the nut until contact with the rim and then tighten to 3.5 ~ 4.5Nm.

- | Tighten slowly with quarter turn steps until the final torque is reached.

- | Do not exceed allowed torque.

- | Do not use electric or pneumatic tools.

4. | Check that the sensor is firmly attached to the rim.

Risk of damage during the tire installation/ removal if the sensor is not firmly attached to the rim.

5. | Carry out inflation / pressure correction and then fit valve cap.

Change the newly installed sensor mode to Normal Fixed Base(Low Line) with the 'GDS'.
Mode (Status / option) of the sensor installed to the vehicle should be Normal Fixed Base (Low).

6. | Install the tire. (Refer to "Tire Installation") Sensor ID Writing (Wireless) Sensor ID Writing