| SONATA(YF) >2012 > G 2.4 GDI > Body (Interior and Exterior) > Seat Belt > Rear Seat Belt>Repair procedures |

Replacement

Rear Seat Belt Replacement

• | When installing the belt, make sure not to damaged the retractor.

1. | Remove the following items first.

A. | Rear seat assembly (Refer to the BD group - "Rear Seat")

B. | Rear Piller trim (Refer to the BD group - "Interior Trim")

2. | After loosening the mounting bolt, then remove the rear seat belt lower anchor (A). [LH,RH]

Tightening torque :
39.2 ~ 53.9 N.m (4.0 ~ 5.5 kgf.m, 28.9 ~ 39.8 lb-ft)

[Center]

Tightening torque :
39.2 ~ 53.9 N.m (4.0 ~ 5.5 kgf.m, 28.9 ~ 39.8 lb-ft)

3. | After loosening the mounting screws, then remove the package tray trim (A).

4. | After loosening the rear seat belt retractor (B) mounting bolt, then remove the rear seat belt (A). [LH,RH]

Tightening torque :
39.2 ~ 53.9 N.m (4.0 ~ 5.5 kgf.m, 28.9 ~ 39.8 lb-ft)

[Center]

Tightening torque :
39.2 ~ 53.9 N.m (4.0 ~ 5.5 kgf.m, 28.9 ~ 39.8 lb-ft)

5. | Installation is the reverse of removal.

Rear Seat Belt Buckle Replacement

1. | Remove the rear seat cushion assembly. (Refer to Rear Seat - "Rear Seat Assembly")

2. | Loosen the mounting bolt, and then remove the rear seat belt buckle (A). [LH]

Tightening torque :
39.2 ~ 53.9 N.m (4.0 ~ 5.5 kgf.m, 28.9 ~ 39.8 lb-ft)

[RH]

Tightening torque :
39.2 ~ 53.9 N.m (4.0 ~ 5.5 kgf.m, 28.9 ~ 39.8 lb-ft)

3. | Installation is the reverse of removal.