| SONATA(YF) >2012 > G 2.4 GDI > Body (Interior and Exterior) > Seat Belt > Front Seat Belt>Repair procedures |

Replacement

Front Seat Belt Replacement

• | When installing the belt, make sure not to damaged the pretensioner.

1. | Remove the following items first :

A. | Front seat assembly (Refer to the BD group - "Front Seat")

B. | Front and rear door scuff trim (Refer to the BD group - "Interior Trim")

2. | Using a screwdriver or remover, remove the seat belt lower anchor (A).

3. | Remove the center pillar lower trim (A).

4. | After loosening the mounting screws, then remove the center pillar upper trim (A) .

5. | After loosening the mounting bolt, then remove the upper anchor (A).

Tightening torque :
39.2 ~ 53.9 N.m (4.0 ~ 5.5 kgf.m, 28.9 ~ 39.8 lb-ft)

6. | After disconnecting the pretensioner connector lock pin, remove the SIS connector (B), loosen the mounting bolt, then remove the pretensioner (A).

Tightening torque :
39.2 ~ 53.9 N.m (4.0 ~ 5.5 kgf.m, 28.9 ~ 39.8 lb-ft)

7. | Installation is the reverse of removal.

Height Adjust Replacement

1. | Remove the following items first :

A. | Front seat assembly (Refer to the BD gruop - "Front Seat")

B. | Front and rear door scuff trim (Refer to the BD gruop - "Interior Trim")

C. | Front seat belt anchor

D. | Center pillar lower trim (Refer to the BD gruop - "Interior Trim")

E. | Center pillar upper trim (Refer to the BD gruop - "Interior Trim")

F. | Front seat belt upper anchor

2. | After loosening the bolts, then remove the hight adjustor (A).

Tightening torque :
39.2 ~ 53.9 N.m (4.0 ~ 5.5kgf.m, 28.9 ~ 39.8 lb-ft)

3. | Installation is the reverse of removal.

• | Replace any damaged clips.

• | Make sure the height adjust properly.

Front Seat Belt Buckle Replacement

1. | Remove the front seat. (Refer to the BD group - "Front Seat")

2. | After loosening the mounting bolt, then remove the front seat belt buckle (A).

Tightening torque :
39.2 ~ 53.9 N.m (4.0 ~ 5.5 kgf.m, 28.9 ~ 39.8 lb-ft)

3. | Installation is the reverse of removal.