| SONATA(YF) >2013 > G 2.4 GDI > Body (Interior and Exterior) > Exterior > Sunroof>Repair procedures |

Replacement

Glass Replacement

- | Put on glove to protect your hands.

1. | Remove the glass (A) by lifting it up.

- | Do not damage the roof panel.

2. | Installation is the reverse of removal.

Motor Replacement

1. | Remove the over head console.

- | Confirm the position of guide whether it is closed or not when you remove the motor.

2. | Disconnect the motor connector (A), remove the screws and then remove the motor (B).

3. | Installation is the reverse of removal.

Deflector Replacement

1. | Open the glass fully.

2. | Disconnect the deflector link (A) from the frame (B), and then remove the deflector (C).

3. | Installation is the reverse of removal.

Sunroof Assembly Replacement

1. | Remove the follows parts.

A. | Front and door scuff trim.

B. | Front, center and rear pillar trim.

C. | Headlining.

D. | Sunroof glass.

2. | Disconnect the drain tubes (A).

3. | After loosening the mounding bolts and nuts, remove the sunroof assembly (B).

- | Take care not to scratch the interior trims and other parts.

4. | Installation is the reverse of removal.

Sunshade And Drip Rail Replacement

1. | Remove the sunroof assembly.

2. | Remove the drip link (A) and sunshade stopper (B).

3. | Remove the sunshade (C) and drip rail (D).

4. | Installation is the reverse of removal.

Guide Assembly Replacement

1. | Remove the sunroof assembly.

2. | Remove a guide assembly (A) after lowering a guide thoroughly by pushing a slide to rear.

3. | Remove the guide (A) and slide (B).

4. | Installation is the reverse of removal.

- | Make sure to align the slide with the center of “A” and “B”

- | Make sure to initialize the motor.

Adjustment

How To Initialize

1. | Check that the glass has been installed.

A. | Finished height adjustment.

2. | Push the down switch. (Keep on pushing the switch)

A. | The slide moved 5mm forward after 15 seconds.

3. | After moving the slide 5mm forward, turn OFF the switch and push the down switch (Keeping on pushing the switch with continuous operation).

A. | If the operation above is normal condition, the sunroof once and closes.

4. | When the sunroof is closed completely, turn OFF the down switch initialize the motor completely.

When To Initialize The Motor

1. | First operation in the vehicle after manufacture it.

2. | Initial value is erased or damaged because of short power electric discharge during operation.

3. | After using the manual (emergency) handle.