| SONATA(YF) >2012 > G 2.4 GDI > Body (Interior and Exterior) > Exterior > Fuel Fill Door>Repair procedures |

Replacement

1. | Remove the fuel fill door cap (A).

2. | After loosening the mounting screws, then remove the fuel fill door catch packing (B).

3. | Detach the clips (A), then remove the fuel fill door (B).

• | Replace fuel fill door housing (C) with new one.

4. | Installation is the reverse of removal.

• | Make sure the fuel fill door locks/unlocks and opens/closes properly.