| SONATA(YF) >2012 > G 2.4 GDI > Engine Control/Fuel System > Fuel Delivery System > Fuel Tank>Repair procedures |

Removal

1. | Release the residual pressure in fuel line (Refer to “Release Residual Pressure in Fuel Line” in this group).

2. | Remove the fuel pump service cover (A) in the trunk.

3. | Disconnect the fuel pump connector (A) and the fuel tank pressure sensor connector (B).

4. | Disconnect the fuel feed tube quick connector (C).

5. | Lift the vehicle and support the fuel tank with a jack.

6. | Remove the center muffler assembly (Refer to “Intake And Exhaust System” in EM group).

7. | Disconnect the fuel filler hose (A), the ventilation tube quick-connector (B), and the vapor tube quick-connector (C,D).

8. | Remove the fuel tank from the vehicle after removing the fuel tank band installation nut (A).

Installation

1. | Installation is reverse of removal.

Fuel tank band installation nut:
39.2 ~ 54.0 N.m (4.0 ~ 5.5 kgf.m, 28.9 ~ 39.8 lb-ft)