| SONATA(YF) >2012 > G 2.4 GDI > Body Electrical System > Sun Roof > Sunroof Motor>Repair procedures |

Inspection

1. | Disconnect the negative (-) battery terminal.

2. | Remove the overhead console and roof trim. (Refer to the BD group - "Roof trim")

3. | Remove the sunroof motor after removing the screws and connector (10P).

4. | Ground the terminals as below table, and check that the sunroof unit operates as below table.

5. | Make these input tests at the connector If any test indicates a problem, find and correct the cause, then recheck the system. If all the input tests prove OK, the sunroof motor must be faulty; replace it.

Terminal | Test condition | Test : Desired result
3 | IG2 ON | Check for voltage to ground : There should be battery voltage
1 | Under all conditions | Check for continuity to ground : There should be continuity.
6 | Under all conditions | Check for voltage to ground : There should be battery voltage.

Resetting The Sunroof
Whenever the vehicle battery is disconnected or discharged, or you use the emergency handle to operate the sunroof, you have to reset your sunroof system as follows :

1. | Turn the ignition key to the ON position.

2. | According to the position of the sunroof, do as follows.

(1) | In case that the sunroof has closed completely or been tilted : Press the TILT button until the sunroof has tilted upward completely.

(2) | In case that the sunroof has slide-opened : Press and hold the CLOSE button for more than 5 seconds until the sunroof has closed completely. Press and hold the CLOSE button for more than 5 seconds after the sunroof has closed completely. Press the TILT button until the sunroof has tilted upward completely.

3. | Release the TILT button.

4. | Press and hold the TILT button once again until the sunroof has returned to the original position of TILT after it is raised a little higher than the maximum TILT position. When this is complete, the sunroof system is reset.

Protecting Motor From Overheating
In order to protect the sunroof motor from overheating from continuous motor operation, the sunroof ECU controls the Run-time and Cool-time of the motor as follows:

1. | The Sunroof ECU detects the Run- time of motor

2. | Motor can be operated continuously for the 1st run-time(120 ± 10sec.).

3. | The continuous operation of motor stops after the 1st Run-time(120 ± 10sec.).

4. | Then Motor is not operated for the 1st Cool-time(18 ± 2sec.).

5. | Motor is operated for the 2nd Run-time(10 ± 2sec.) at the continued motor operation after 1st Cool-time(18 ± 2sec.)

6. | The continuous operation of motor stops operating after the 2nd Run-time(10 ± 2sec.)

7. | Motor is not operated for the 2nd Cool-time(18 ± 2sec.).

8. | Motor repeats the 2nd run-time and 2nd cool-time at the continued motor operation.

A. | In case that motor is not operated continuously, the run-time is increased.

B. | The Run-Time of motor is initialized to "0" if the battery or fuse is reconnected after being disconnected, discharged or blown.

T1 : 120 ± 10 sec., T2 : 18 ± 2 sec.,
T3 : 10 ± 2 sec., T4 : 18 ± 2 sec.