| SONATA(YF) >2013 > G 2.4 GDI > Suspension System > General Information>Specifications |

Specifications

Front Suspension

Item | Specification
Suspension type | MacPherson Strut
Shock absorber | Type | Gas
Coil spring | Free Height [I.D. color] | 311.8mm (12.28 in.) [White - Green]
282.8mm (11.13 in.) [White - Yellow]

Rear Suspension

Item | Specification
Suspension type | Multi link
Shock absorber | Type | Gas
Coil spring | Free Height [I.D. color] | 300.4mm (11.83 in.) [White - Green]
294.8mm (11.61 in.) [White - Yellow]

Wheel & Tire

Item | Specification
Wheel | 6.5J * 16, 43 (Wheel off set)
6.5J * 17, 46 (Wheel off set)
7.5J * 18, 48 (Wheel off set)
Tire | P205/ 65 R16
P215/ 55 R17
225/ 45 R18
Tire pressure | P205/ 65R16 | 2.3+0.07kg/cm² (33+1.0psi)
P215/ 55R17 | 2.3+0.07kg/cm² (33+1.0psi)
225/ 45R18 | 2.5+0.07kg/cm² (35+1.0psi)
T125/ 80D16 | 4.2+0.07kg/cm² (60+1.0psi)

Wheel Alignment

Front

Item | Specification
Front | Rear
Toe-in | Total | 0.16°±0.2° | 0.17±0.2°
Individual | 0.08°±0.1° | 0.085°±0.1°
Camber angle | -0.5°±0.5° | -1.0°±0.5°
Caster angle | 4.44°±0.5° | -
King-pin angle | 12.73°±0.5° | -

Tightening Torque

Front Suspension

Item | Tightening torque
Nm | kgf.m | lb-ft
Hub nuts | 88.3 ~ 107.9 | 9.0 ~ 11.0 | 65.1 ~ 79.6
Strut assembly to knuckle | 137.3 ~ 156.9 | 14.0 ~ 16.0 | 101.3 ~ 115.7
Strut assembly lock nut | 44.1 ~ 58.8 | 4.5 ~ 6.0 | 32.5 ~ 43.4
Stabilizer link to strut assembly | 98.1 ~ 117.7 | 10.0 ~12.0 | 72.3 ~ 86.8
Lower arm to sub frame (Front) | 137.3 ~ 156.9 | 14.0 ~16.0 | 101.3 ~ 115.7
Lower arm to sub frame (Rear) | 98.1 ~ 117.7 | 10.0 ~12.0 | 72.3 ~ 86.8
Lower arm to knuckle | 98.1 ~ 117.7 | 10.0 ~12.0 | 72.3 ~ 86.8
Stabilizer bar to stabilizer link | 98.1 ~ 117.7 | 10.0 ~ 12.0 | 72.3 ~ 86.8
Stabilizer bracket mounting bolts | 49.0 ~ 63.7 | 5.0 ~ 6.5 | 36.2 ~ 47.0
Cross member to body | 156.9 ~ 176.5 | 16.0 ~ 18.0 | 115.7 ~ 130.2
Tie rod end castle nut | 34.3 ~ 44.1 | 3.5 ~ 4.5 | 25.3 ~ 32.5
Universal joint to pinion of steering gear | 32.4 ~ 37.3 | 3.3 ~ 3.8 | 23.9 ~ 27.5

Rear Suspension

Item | Tightening torque
Nm | kgf.m | lb-ft
Hub nuts | 88.3 ~ 107.9 | 9.0 ~ 11.0 | 65.1 ~ 79.6
Trailing arm to body | 98.1 ~ 117.7 | 10.0 ~12.0 | 72.3 ~ 86.8
Trailing arm to knuckle | 44.1 ~ 53.9 | 4.5 ~ 5.5 | 32.5 ~ 39.8
Assist arm to sub frame | 107.9 ~ 117.7 | 11.0 ~ 12.0 | 79.6 ~ 86.8
Assist arm to knuckle | 78.5 ~ 88.3 | 8.0 ~ 9.0 | 57.9 ~ 65.1
Lower arm to sub frame | 107.9 ~ 117.7 | 11.0 ~ 12.0 | 79.6 ~ 86.8
Lower arm to knuckle | 137.3 ~ 156.9 | 14.0 ~ 16.0 | 101.3 ~ 115.7
Upper arm to sub frame | 137.3 ~ 156.9 | 14.0 ~ 16.0 | 101.3 ~ 115.7
Upper arm to knuckle | 137.3 ~ 156.9 | 14.0 ~ 16.0 | 101.3 ~ 115.7
Shock absorber to frame | 49.0 ~ 63.7 | 5.0 ~ 6.5 | 36.2 ~ 47.0
Shock absorber to knuckle | 137.3 ~ 156.9 | 14.0 ~ 16.0 | 101.3 ~ 115.7
Stabilizer bar to stabilizer link | 98.1 ~ 117.7 | 10.0 ~ 12.0 | 72.3 ~ 86.8
Stabilizer bar to sub frame | 44.1 ~ 53.9 | 4.5 ~ 5.5 | 32.5 ~ 39.8
Sub frame mounting bolt & nut | 156.9 ~ 176.5 | 16.0 ~ 18.0 | 115.7 ~ 130.2