| SONATA(YF) >2012 > G 2.4 GDI > Body Electrical System > Audio > Multimedia jack>Repair procedures |

Removal

1. | Remove the shift lever knob. (Refer to the BD group - "Console")

2. | Remove the console upper cover (A).

3. | Disconnect the connector (A) from the console upper cover.

4. | Remove the multimedia jack (B) from the console under cover after releasing the fixed hooks (A).

Installation

1. | Install the multimedia jack.

2. | Connect the multimedia jack connector.

3. | Install the console upper cover.

4. | Install the shift lever knob.

Make sure the multimedia connector and the console upper cover connectors are plugged in properly.