| SONATA(YF) >2013 > G 2.4 GDI > Automatic Transaxle System > Automatic Transaxle Control System > Transaxle Oil Temperature Sensor>Repair procedures |

Removal

1. | Remove the battery and the battery tray. (Refer to "Charging system" in EE group.)

2. | Remove the under cover (A).

3. | Replace new gasket and the plug after drining the automatic transaxle fluid by removing the drain plug. (Refer to "Automatic transaxle system" in this group.)

4. | Remove the valve body cover (A) and eyebolt (B).

Tightening torque:
(A) 12.8 ~ 14.7 N.m (1.3 ~ 1.5 kgf.m, 9.4 ~ 10.8 lb-ft)
(B) 34.3 ~ 44.1 N.m (3.5 ~ 4.5 kgf.m, 25.3 ~ 32.6 lb-ft)

The gasket of the eyebolt use new one.

Remove installation bolts in the engin room first and then remove others under the vehicle.

5. | Disconnect the oil temperature sensor connector (A).

6. | Remove the oil temperature sensor (A) after removing a bolt.

Tightening torque:
9.8 ~ 11.8 N.m (1.0 ~ 1.2 kgf.m, 7.2 ~ 8.7 lb-ft)

Be careful not to damage the harness lock connector.

Installation

1. | Installation is the reverse of removal.

After replacement or reinstallation procedure of the valve body assembly, must perform procedures below.

• | Continue to apply liquid gasket at application points at the valve body cover with Ø2.5mm (0.0984in.) thickness.

Liquid gasket Part name :
Threebond 1281B or LOCTITE FMD-546

• | Adding automatic transaxle fluid. (Refer to "automatic transaxle system" in this group.)