| SONATA(YF) >2012 > G 2.4 GDI > Body Electrical System > Lighting System > High Mounted stop lamp>Repair procedures |

Removal

1. | Disconnect the negative(-) battery terminal.

2. | Remove the rear seat. (Refer to the BD group - "Rear seat")

3. | Disconnect the connector of high mounted stop lamp.

4. | Remove the package tray trim (A). (Refer to the BD group -"Interior trim")

5. | Remove the high mounted stop lamp.

Installation

1. | Install the high mounted stop lamp to the rear package tray.

2. | Install the rear package tray trim.

3. | Install the rear seat.