| SONATA(YF) >2013 > G 2.4 GDI > Heating,Ventilation, Air Conditioning > Blower > Blower Motor>Repair procedures |

Inspection

1. | Connect the battery voltage and check the blower motor rotation.

2. | If the blower motor voltage is not operated well, substitute with a known-good blower motor and check for proper operation.

3. | If the problem is corrected, replace the blower motor.

Replacement

1. | Disconnect the negative (-) battery terminal.

2. | Remove the crash pad lower panel (A).

3. | Disconnect the of the blower motor connector (A).

4. | Remove the blower motor (B) by pulling it after rotating 90° in a counter clock wise direction.

5. | Installation is the reverse order of removal.