| SONATA(YF) >2013 > G 2.4 GDI > Body Electrical System > Back View Camera System>Repair procedures |

Removal

Back View Camera

1. | Remove the screws, clip and trunk lid trim in the trunk. (Refer to the BD group - "Trunk Lid")

2. | Remove the trunk lid garnish.

3. | Remove the back view camera (A) after removing the connector and screws.

Back View Camera Unit

1. | Disconnect the negative (-) battery terminal.

2. | Remove glove box housing. (Refer to BD group - "Crash Pad")

3. | Remove the back view camera unit (A) after removing the nut and connector.

Installation

Back View Camera

1. | Install the back view camera.

2. | Install the trunk lid garnish and trim.

Back View Camera Unit

1. | Install the front back view camera unit.

2. | Install the glove box and housing.

3. | Connect the negative (-) battery terminal.