| SONATA(YF) >2013 > G 2.4 GDI > Engine Control/Fuel System > Engine Control System > Fuel Tank Pressure Sensor (FTPS)>Repair procedures |

Inspection

1. | Connect the GDS on the Data Link Connector (DLC).

2. | Measure the output voltage of the FTPS.

Specification: Refer to "Specification"

Removal

1. | Turn the ignition switch OFF and disconnect the battery negative (-) cable.

2. | Remove the fuel pump service cover (A) in the trunk.

3. | Disconnect the fuel tank pressure sensor connector (A), and then remove the fuel tank pressure sensor.

Installation

• | Install the component with the specified torques.

• | Note that internal damage may occur when the component is dropped. If the component has been dropped, inspect before installing.

• | Insert the sensor in the installation hole and be careful not to damage.

1. | Installation is reverse of removal.