| SONATA(YF) >2013 > G 2.4 GDI > Engine Control/Fuel System > Engine Control System > Variable Intake Solenoid (VIS) Valve>Description and Operation |

Description

Variable Intake manifold Solenoid (VIS) valve is installed on the intake manifold. The VIS valve controls the vacuum modulator which activates a valve in the intake manifold. The ECM opens or closes this valve according to engine condition (Refer to below table).

Engine condition | VIS valve | Operation
Medium speed | Closed | Increasing engine performance in low engine speed by reducing intake interference among cylinders
Low / High speed | Open | Minimizing intake resistance by shortening intake manifold length and increasing area of air entrance