| SONATA(YF) >2012 > G 2.4 GDI > Manual Transaxle System > Manual Transaxle System>Repair procedures |

Service Adjustment Procedure

Transmission Oil Inspection And Replacement

1. | Park the vehicle on a level ground and stop the engine.

2. | Remove the oil filler plug and washer. Inspect the manual transaxle fluid condition and quantity.

3. | If the manual transaxle fluid is contaminated, drain it out by removing the oil drain plug.

4. | Tighten the new oil drain plug(A) and fill manual transaxle fluid to a proper level.

Tightening torque :
(A) 58.9~78.5N.m (6.0~8.0kgf.m, 43.4~57.9lb-ft)

Oil type: SAE75W/85
Oil quantity: 1.8L(0.48 U.S.gal., 1.90 U.S. qt., 1.58 lmp.qt.)

5. | Retighten the oil filler plug(B) with a new washer.

Tightening torque :
(B) 29.4~34.3N.m (3.0~3.5kgf.m, 21.7~25.3lb-ft)

Back Up Lamp Switch Inspection

1. | Disconnect the back up lamp switch connector (A).

2. | Inspect the continuity of the switch. When the shift lever is in reverse range, it should have continuity.

3. | Replace the back up lamp switch, if necessary.

Tightening torque :
29.4~34.4 N.m (3.0~3.5Kgf.m, 21.7~25.3lb-ft)