| SONATA(YF) >2012 > G 2.4 GDI > Restraint > SRSCM > Seat Track Position Sensor (STPS)>Repair procedures |

Removal

1. | Disconnect the battery negative cable, and wait for at least three minutes before beginning work.

2. | Remove the front seat assembly. (Refer to BD group)

3. | Loosen the two STPS screws, then remove the STPS after disconnecting the STPS connector.

Installation

Be sure to install the harness wires so they will not pinch or interfere with other parts.

1. | Remove the ignition key from the vehicle.

2. | Disconnect the battery negative cable, and wait for at least three minutes before beginning work.

3. | Install the STPS with two screws.

4. | Install the front seat assembly. (Refer to BD group)

5. | Reconnect the battery negative cable.

6. | After installing the Seat Track Position Sensor, confirm proper system operation: Turn the ignition switch ON, the SRS indicator should be turned on for about six seconds and then go off.