| SONATA(YF) >2013 > G 2.4 GDI > Engine Control/Fuel System > Engine Control System > Manifold Absolute Pressure Sensor (MAPS)>Repair procedures |

Inspection

1. | Connect the GDS on the Data Link Connector (DLC).

2. | Measure the output voltage of the MAPS at idle and IG ON.

Specification: Refer to "Specification"

Removal

1. | Turn the ignition switch OFF and disconnect the battery negative (-) cable.

2. | Disconnect the manifold absolute pressure sensor connector (A).

3. | Remove the installation bolt (B), and then remove the sensor from the surge tank.

Installation

• | Install the component with the specified torques.

• | Note that internal damage may occur when the component is dropped. If the component has been dropped, inspect before installing.

• | Insert the sensor in the installation hole and be careful not to damage.

1. | Installation is reverse of removal.

Manifold absolute pressure sensor installation bolt:
9.8 ~ 11.8 N.m (1.0 ~ 1.2 kgf.m, 7.2 ~ 8.7 lb-ft)