| SONATA(YF) >2013 > G 2.4 GDI > Body Electrical System > Button Engine Start System > Fob Holder>Repair procedures |

Removal

1. | Disconnect the negative(-) battery terminal.

2. | Remove the floor console. (Refer to the BD group - "Console")

3. | Disconnect the fob holder connector (A).

4. | Remove the fob holder (A) by pushing both sides of the hooks.

Installation

1. | Install the fob holder.

2. | Install the floor console.