| SONATA(YF) >2012 > G 2.4 GDI > Body Electrical System > Seat Electrical > Power Seat Control Switch>Repair procedures |

Inspection

With the power seat switch in each position, make sure that continuity exists between the terminals below. If continuity is not as specified, replace the power seat switch.
A : Power seat control switch
B : Lumber support switch

Removal

1. | Disconnect the negative (-) battery terminal.

2. | Remove the seat side cover (A). (Refer to the BD group - "Front seat")

3. | Disconnect the power seat control switch connector (A).

4. | Loosen the power seat control switch (A) mounting screws (3EA).

Installation

- | Make sure that the IMS control switch connectors and related connectors are plugged in properly.

- | Check the IMS control switch operates normally.

1. | Connect the connectors and reassemble the IMS control switch.

2. | Reassemble the seat side cover.