| SONATA(YF) >2012 > G 2.4 GDI > Body (Interior and Exterior) > Exterior > Trunk Lid>Repair procedures |

Replacement

Trunk Lid Assembley Replacement

• | When removing and installing the trunk lid, an assistant is necessary.

• | Wear gloves to protect hands from injury.

1. | Remove the trunk inside hondle cover (B).

2. | After loosening the mounting screws, then remove the trunk inside handle (A).

3. | Detach the clips, then remove the trunk lid trim (A).

4. | Disconnect wiring the connectors.

5. | After loosening the mounting bolts, then remove the trunk lid (A).

Tightening torque:
6.9~8.8 N.m (0.7~0.9 kgf.m, 5.1~6.5 lb-ft)

6. | Installation is the reverse of removal.

• | Replace any damaged clips.

Trunk Lid Weatherstrip Replacement

1. | Remove the trunk lid weatherstrip (A).

2. | Installation is the reverse of removal.

Key Holder Replacement

1. | Remove the trunk lid trim.

2. | Disconnect the inside handle cable (A), then loosen the key holder (B) mounting bolts and remove.

3. | Installation is the reverse of removal.

Trunk Lid Latch Replacement

1. | Remove the trunk lid trim.

2. | Disconnect the connector (A).

3. | Disconnect the cable (B), then loosen the latch assembly (C) mounting bolts and remove.

4. | Installation is the reverse of removal.

Adjustment

1. | After loosening the trunk lid hinge (A) mounting bolt, adjust the trunk lid by moving it up or down, or right or left.

2. | Adjust the trunk lid height by turning the trunk lid overslam bumpers (B).

3. | After loosening the trunk lid latch (C) mounting bolts, adjust the trunk lid latch by moving it up or down, or right or left.