| SONATA(YF) >2013 > G 2.4 GDI > Steering System > Steering wheel > Flex Steer>Repair procedures |

Inspection

1. | Check the audio remote control switch for resistance between terminals in each switch position.

Switch | Connector terminal | Resistance[KΩ]
Flex | 3-4 | 1.44±5%
Trip | 3-5 | 2.54±5%
RESET | 3-4 | 5.54±5%

Removal

1. | Disconnect the negative (-) battery terminal.

2. | Remove the driver airbag module. (Refer to Restraint - "Driver Airbag (DAB) Module and Clock Spring")

3. | Remove the steering wheel. (Refer to Steering Wheel - "Steering wheel ")

4. | Loosen the screw and then romove the steering wheel switch connector.