| SONATA(YF) >2012 > G 2.4 GDI > Engine Control/Fuel System > General Information>Specifications |

Specifications

Fuel Delivery System

Items | Specification
Fuel Tank | Capacity | 70 lit. (18.5 U.S.gal., 74.0 U.S.qt., 61.6 Imp.qt.)
Fuel Filter | Type | Paper type
Fuel Pressure | Low Pressure Fuel Line | 480 ~ 520 kPa (4.9 ~ 5.3 kgf/cm², 69.6 ~ 75.4 psi)
High Pressure Fuel Line | 2.0 ~ 15.0 MPa (20.4 ~ 153.0 kgf/cm², 290.1 ~ 2175.6 psi)
Fuel Pump | Type | Electrical, in-tank type
Driven by | Electric motor
High Pressure Fuel Pump | Type | Mechanical type
Driven by | Camshaft

Sensors

Manifold Absolute Pressure Sensor (MAPS)
▷ Type: Piezo-resistive pressure sensor type
▷ Specification

Pressure [kPa (kgf/cm², psi)] | Output Voltage (V)
20.0 (0.20, 2.9) | 0.79
46.7 (0.47, 6.77) | 1.84
101.3 (1.03, 14.7) | 4.0

Intake Air Temperature Sensor (IATS)
▷ Type: Thermistor type
▷ Specification

Temperature | Resistance (kΩ)
°C | °F
-40 | -40 | 40.93 ~ 48.35
-20 | -4 | 13.89 ~ 16.03
0 | 32 | 5.38 ~ 6.09
10 | 50 | 3.48 ~ 3.90
20 | 68 | 2.31 ~ 2.57
40 | 104 | 1.08 ~ 1.21
50 | 122 | 1.56 ~ 1.74
60 | 140 | 0.54 ~ 0.62
80 | 176 | 0.29 ~ 0.34

Engine Coolant Temperature Sensor (ECTS)
▷ Type: Thermistor type
▷ Specification

Temperature | Resistance (kΩ)
°C | °F
-40 | -40 | 48.14
-20 | -4 | 14.13 ~ 16.83
0 | 32 | 5.79
20 | 68 | 2.31 ~ 2.59
40 | 104 | 1.15
60 | 140 | 0.59
80 | 176 | 0.32

Throttle Position Sensor (TPS) [integrated into ETC Module]
▷ Type: Variable resistor type
▷ Specification

Throttle Angle(°) | Output Voltage (V)
TPS1 | TPS2
0 | 0 | 5.0
10 | 0.48 | 4.52
20 | 0.95 | 4.05
30 | 1.43 | 3.57
40 | 1.90 | 3.10
50 | 2.38 | 2.62
60 | 2.86 | 2.14
70 | 3.33 | 1.67
80 | 3.81 | 1.19
90 | 4.29 | 0.71
100 | 4.76 | 0.24
105 | 5.0 | 0
C.T (6~15°) | 0.29 ~ 0.71 | 4.29 ~ 4.71
W.O.T (93~102°) | 4.43 ~ 4.86 | 0.14 ~ 0.57

Item | Resistance (kΩ)
TPS1 | 0.875 ~ 1.625 [20°C(68°F)]
TPS2 | 0.875 ~ 1.625 [20°C(68°F)]

Crankshaft Position Sensor (CKPS)
▷ Type: Hall effect type
Camshaft Position Sensor (CMPS)
▷ Type: Hall effect type
Knock Sensor (KS)
▷ Type: Piezo-electricity type
▷ Specification

Item | Specification
Capacitance (pF) | 850 ~ 1,150

Heated Oxygen Sensor (HO2S) [Bank 1/Sensor 1]
▷ Type: Zirconia (ZrO2) [Linear] Type
▷ Specification

Item | Specification
Heater Resistance (Ω) | 2.5 ~ 4.0 [20°C(69.8°F)]

Heated Oxygen Sensor (HO2S) [Bank 1/Sensor 2]
▷ Type: Zirconia (ZrO2) [Binary] Type
▷ Specification

A/F Ratio (λ) | Output Voltage(V)
RICH | Approx. 0.9
LEAN | Approx. 0.04

Item | Specification
Heater Resistance (Ω) | 3.3 ~ 4.1 [21°C(69.8°F)]

Rail Pressure Sensor (RPS)
▷ Type: Piezo-electricity type
▷ Specification

Accelerator Position Sensor (APS)
▷ Type: Variable resistor type
▷ Specification

Accelerator Position | Output Voltage (V)
APS1 | APS2
C.T | 0.7 ~ 0.8 | 0.29 ~ 0.46
W.O.T | 3.85 ~ 4.35 | 1.93 ~ 2.18

Fuel Tank Pressure Sensor (FTPS)
▷ Type: Piezo - Resistivity type
▷ Specification

Pressure [kPa (kgf/cm², in H2O) | Output Voltage (V)
-6.67 (-0.068, -26.8) | 0.5
0 | 2.5
+6.67 (0.068, 26.8) | 4.5

Actuators

Injector
▷ Specification

Item | Specification
Coil Resistance (Ω) | 1.18 ~ 1.31 [20°C(68°F)]

ETC Motor [integrated into ETC Module]
▷ Specification

Item | Specification
Coil Resistance (Ω) | 1.2 ~ 1.8 [20°C(68°F)]

Purge Control Solenoid Valve (PCSV)
▷ Specification

Item | Specification
Coil Resistance (Ω) | 19.0 ~ 22.0 [20°C(68°F)]

CVVT Oil Control Valve (OCV)
▷ Specification

Item | Specification
Coil Resistance (Ω) | 6.9 ~ 7.9 [20°C(68°F)]

Variable Intake Solenoid (VIS) Valve
▷ Specification

Item | Specification
Coil Resistance (Ω) | 30.0 ~ 35.0 [20°C(68°F)]

Fuel Pressure Regulator Valve
▷ Specification

Item | Specification
Coil Resistance (Ω) | 0.5 [20°C(68°F)]

Ignition Coil
▷ Type: Stick type
▷ Specification

Item | Specification
Primary Coil Resistance (Ω) | 0.62 ± 10％[20°C(68°F)]
Secendary Coil Resistance (kΩ) | 7.0 ± 15％[20°C(68°F)]

Canister Close Valve (CCV)
▷ Specification

Item | Specification
Coil Resistance (Ω) | 19.9 ~ 22.9 [20°C(68°F)]

Service Standard

Item | Specification
Ignition Timing (°) | BTDC 6 ± 10
Idle Speed (rpm) | A/C OFF | Neutral, N, P-range | 600 ± 100
D-range | 600 ± 100
A/C ON | Neutral, N, P-range | 600 ± 100
D-range | 600 ± 100

Tightening Torques

Engine Control System

Item | kgf.m | N.m | lb-ft
ECM installation bolt | 1.0 ~ 1.2 | 9.8 ~ 11.8 | 7.2 ~ 8.7
ECM bracket installation bolt/nut | 1.0 ~ 1.2 | 9.8 ~ 11.8 | 7.2 ~ 8.7
Manifold absolute pressure sensor installation bolt | 1.0 ~ 1.2 | 9.8 ~ 11.8 | 7.2 ~ 8.7
Crankshaft position sensor installation bolt | 1.0 ~ 1.2 | 9.8 ~ 11.8 | 7.2 ~ 8.7
Crankshaft position sensor cover installation bolt (M6) | 1.0 ~ 1.2 | 9.8 ~ 11.8 | 7.2 ~ 8.7
Crankshaft position sensor cover installation bolt (M8) | 1.9 ~ 2.4 | 18.6 ~ 23.5 | 13.7 ~ 17.4
Camshaft position sensor (Bank 1 / Intake) installation bolt | 1.0 ~ 1.2 | 9.8 ~ 11.8 | 7.2 ~ 8.7
Camshaft position sensor (Bank 1 / Exhaust) installation bolt | 1.0 ~ 1.2 | 9.8 ~ 11.8 | 7.2 ~ 8.7
Knock sensor installation bolt | 1.9 ~ 2.4 | 18.6 ~ 23.5 | 13.7 ~ 17.4
Heated oxygen sensor (Bank 1 / sensor 1) installation | 4.0 ~ 5.0 | 39.2 ~ 49.1 | 28.9 ~ 36.2
Heated oxygen sensor (Bank 1 / sensor 2) installation | 4.0 ~ 5.0 | 39.2 ~ 49.1 | 28.9 ~ 36.2
Rail pressure sensor installation | 1.8 ~ 2.2 | 18.0 ~ 22.0 | 13.3 ~ 16.2
Electronic throttle body installation bolt | 0.8 ~ 1.2 | 7.8 ~ 11.8 | 5.8 ~ 8.7
Purge control solenoid valve bracket installation bolt | 1.0 ~ 1.2 | 9.8 ~ 11.8 | 7.2 ~ 8.7
CVVT oil control valve (Bank 1 / Intake) installation bolt | 1.0 ~ 1.2 | 9.8 ~ 11.8 | 7.2 ~ 8.7
CVVT oil control valve (Bank 1 / Exhaust) installation bolt | 1.0 ~ 1.2 | 9.8 ~ 11.8 | 7.2 ~ 8.7
Ignition coil installation bolt | 1.0 ~ 1.2 | 9.8 ~ 11.8 | 7.2 ~ 8.7

Fuel Delivery System

Item | kgf.m | N.m | lb-ft
Fuel tank installation nut | 4.0 ~ 5.5 | 39.2 ~ 54.0 | 28.9 ~ 39.8
Filler-neck assembly bracket installation bolt | 0.4 ~ 0.6 | 3.9 ~ 5.9 | 2.9 ~ 4.3
Accelerator pedal module installation nut | 1.0 ~ 1.5 | 9.8 ~ 14.7 | 7.2 ~ 10.8
Accelerator pedal module installation bolt | 0.9 ~ 1.4 | 8.8 ~ 13.7 | 6.5 ~ 10.1
Delivery pipe installation bolt | 1.9 ~ 2.4 | 18.6 ~ 23.5 | 13.7 ~ 17.4
High pressure fuel pump installation bolt | 1.3 ~ 1.5 | 12.8 ~ 14.7 | 9.4 ~ 10.9
High pressure fuel pipe installation nut | 2.7 ~ 3.3 | 26.5 ~ 32.4 | 19.5 ~ 23.9
High pressure fuel pipe function block installation bolt | 0.8 ~ 1.2 | 7.8 ~ 11.8 | 5.8 ~ 8.7