| SONATA(YF) >2012 > G 2.4 GDI > Body Electrical System > Power Door Locks > Power Door Lock Switch>Repair procedures |

Inspection

Driver Door Lock Switch Inspection

1. | Disconnect the negative (-) battery terminal.

2. | Remove the front door trim panel. (Refer to the BD group - "Front door")

3. | Disconnect the connector from the power window switch module.

4. | Check for continuity between the terminals in each switch position according to the table.

Removal

1. | Disconnect the negative(-) battery terminal.

2. | Remove the front door trim panel. (Refer to the BD group - "Front door")

3. | Disconnect the power window switch module connector (A) from the wiring harness.

4. | Remove the power window switch module (A) from the door trim after loosening the mounting screws (11EA).

5. | Remove the module from the sub box assembly after loosening the mounting screw (1EA).

- | Be careful not to damage door trim panel and door module mounting hooks.

Installation

1. | Install the power window switch module.

2. | Install the door trim panel after reconnecting the relevant connectors

- | Make sure that the power window switch module connectors are plugged properly.

- | Check that the power window switch and door lock switch operate normally.