| SONATA(YF) >2012 > G 2.4 GDI > Body Electrical System > Back View Camera System>Description and Operation |

Description

Back view camera will activate when the backup light is ON with the ignition switch ON and the shift lever in the R position.
This system is a supplemental system that shows behind the vehicle through the AV monitor while backing-up.

This system is a supplementary function only. It is the responsibility of the driver to always check the inside/ outside rearview mirror and the area behind the vehicle before and during backing up because there are blind spots that can't be seen through the camera.