| SONATA(YF) >2013 > G 2.4 GDI > Body Electrical System > Power Door Locks > Power Door Lock Relay>Repair procedures |

Inspection

1. | Disconnect the negative (-) battery terminal.

2. | Remove the junction box.

3. | Check for continuity between the terminals. [Front] [Rear]

Door Lock

1. | There should be continuity between the No.38 terminal in the I/P-E and No.21(or 34) terminal in the I/P-A when power and ground are connected to the No.38 terminal in the I/P-E and ground.

2. | There should be no continuity between the No.38 terminal in the I/P-E and No.21(or 34) terminal in the I/P-A when power is disconnected.

Door Unlock

1. | There should be continuity between the No.38 terminal in the I/P-E and No.22(or 35) terminal in the I/P-A when power and ground are connected to the No.38 terminal in the I/P-E and ground.

2. | There should be no continuity between the No.38 terminal in the I/P-E and No.22(or 35) terminal in the I/P-E when power is disconnected.

Trunk Lid Open

1. | There should be continuity between the No.1 terminal in the I/F-C and No.36 terminal in the I/F-A when power and ground are connected to the No.1 terminal in the I/F-C and ground.

2. | There should be no continuity between the No.1 terminal in the I/F-C and No.36 terminal in the I/F-A when power is disconnected.

Diagnosis With GDS

1. | It will be able to diagnose defects of power door lock with GDS quickly. GDS can operates actuator forcefully, input/output value monitoring and self diagnosis.

2. | Select model and "BCM".

3. | Select the "SJB" to check.

4. | Select "Current data", if you will check current data of power door lock system. It provides input/output status of SJB.

5. | If you will check the power door lock operation forcefully, select "Actuation test".