| SONATA(YF) >2012 > G 2.4 GDI > Body Electrical System > Fuses And Relays > The Other Fuses And Relays Component>Repair procedures |

Inspection

Power Relay Test (Type B)
Check for continuity between the terminals.
A : Two turn unlock relay

1. | There should be continuity between the No.30 and No.87 terminals when power and ground are connected to the No.85 and No.86 terminals.

2. | There should be continuity between the No.30 and No.87 terminals when power is disconnected.