| SONATA(YF) >2013 > G 2.4 GDI > Engine Control/Fuel System > Fuel Delivery System > Filler-Neck Assembly>Repair procedures |

Removal

1. | Disconnect the fuel filler hose (A), the vapor tube quick-connector (B), and the ventilation tube quick-connector (C).

2. | Remove the rear-LH wheel, tire, and the inner wheel house.

3. | Open the fuel filler door and unfasten the filler-neck assembly mounting screw (A).

4. | Remove the filler-neck assembly from the vehicle after removing the bracket mounting bolts (A).

Installation

1. | Installation is reverse of removal.

Filler-neck assembly bracket installation bolt :
3.9 ~ 5.9 N.m (0.4 ~ 0.6 kgf.m, 2.9 ~ 4.3 lb-ft)