| SONATA(YF) >2013 > G 2.4 GDI > Suspension System > Rear Suspension System > Rear Shock Absorber>Repair procedures |

Replacement

1. | Remove the rear wheel & tire.

Tightening torque:
88.3 ~ 107.9 N.m (9.0 ~ 11.0 kgf.m, 65.1 ~ 79.6 lb-ft)

Be careful not to damage to the hub bolts when removing the rear wheel & tire.

2. | Loosen the bolt & nut and then disconnect the shock absorber (A) with the rear axle.

Tightening torque:
137.3~156.9 N.m (14.0~16.0 kgf.m, 101.3~115.7 lb-ft)

3. | Loosen the shock absorber mounting bolts (A).

Tightening torque:
49.0 ~ 63.7 N.m (5.0 ~ 6.5 kgf.m, 36.2 ~ 47.0 lb-ft)

4. | Installation is the reverse of removal.

Inspection

1. | Check the rubber parts for wear and deterioration.

2. | Compress and extend the piston rod (A) and check that there is no abnormal resistance or unusual sound during operation.