This driver needs a file. It is called .MIX

Is very important to create manually the file .MIX

Instructions to create a .MIX for BMW 320d

We image the file with 16 bit ( LL + HH ), at the address in the table, is important replace the value (in ORI cell) with the value of MIX cell.

Ecu (there's written 205 on the label)

Address | ORI | MIX
#3BA45 | 23 | 2C
#3BA47 | 2A | 37

Ecu 445 eprom 098

Address | ORI | MIX
#3BB0F | 23 | 2C
#3BB11 | 2A | 37

Ecu 445 eprom 326

Address | ORI | MIX
#3BAEB | 23 | 2C
#3BAED | 2A | 37

Ecu 445 eprom 344

Address | ORI | MIX
#3BA45 | 23 | 2C
#3BA47 | 2A | 37

Ecu 445 eprom 420

Address | ORI | MIX
#3BA45 | 23 | 2C
#3BA47 | 2A | 37

Ecu 445 eprom 731

Address | ORI | MIX
#3BA4B | 23 | 2C
#3BA4D | 2A | 37

Ecu 445 eprom 863

Address | ORI | MIX
#3BB0F | 23 | 2C
#3BB11 | 2A | 37

Ecu 445 eprom 887

Address | ORI | MIX
#3BA45 | 23 | 2C
#3BA47 | 2A | 37

Ecu 445 eprom 970

Address | ORI | MIX
#3BAEB | 23 | 2C
#3BAED | 2A | 37