| SONATA(YF) >2013 > G 2.4 GDI > Body Electrical System > Hands Free System>Description and Operation |

Function

Audio Bluetooth System

General Feature

• | This audio system supports Bluetooth®hands-free and stereo-headset features. - HANDS-FREE feature: Making orreceiving calls wirelessly throughvoice recognition.

• | The phone must be paired to the system before using the hands-free feature. - STEREO-HEADSET feature: Playingmusic from cellular phones (that supportsA2DP feature) wirelessly.

• | Voice recognition engine of theBluetooth® system supports 3 types oflanguages: - English - US Spanish - Canadian French

If the vehicle is moving do not use a cellular phone or connect the Bluetooth phone.

• | The phone must be paired to the systembefore using Bluetooth® features.

• | Only one selected (linked) cellularphone can be used with the system ata time.

• | Some phones are not fully compatiblewith this system.

Voice Recognition Activation

• | The voice recognition engine contained in the Bluetooth System can be activated in the following conditions: - Button Activation The voice recognition system will be active when the button is pressed and after the sound of a Beep. - Active Listening
The voice recognition system will beactive for a period of time when the Voice Recognition system has asked for a customer response.

• | The system can recognize single digits from zero to nine while number greater than ten will not be recognized.

• | If the command is not recognized, the system will announce "Pardon" or No input voice signal from microphone. (Noresponse)

• | The system shall cancel voice recogntionmode in following cases : When pressing the button and saying cancel following the beep. When not making a call and pressing the button. When voice recognition has failed 3 consecutive times.

• | At any time if you say "help", the system will announce what commands are available.

Menu tree

Phone Setup
All Bluetooth® related operations can beperformed by voice command or by manualoperation.

• | By Voice Command: Press button on the steeringwheel to activate voice recognition.

Push the TUNE knob to enter SETUPmode.Select desired item by pressing the [∨ FOLDER ∧] button, then push the[ENTER] button.Select “BT” item by rotating the TUNEknob, then push the knob.Select desired item by rotating the TUNEknob, then push the knob.
Press the [SET UP] button to enterSETUP MODE.Select "BLUETOOTH" item by pressingthe [∨ FOLDER ∧] button, then pushthe [ENTER] button.

Pairing phone

Before using Bluetooth® features, thephone must be paired (registered) to theaudio system. Up to 5 phones can bepaired in the system.

1. | Press button.

2. | Say "Set Up". - The system replies with availablecommands. - To skip the information message, press again and then a beep isheard.

3. | Say "Pair Phone".

4. | Say “Yes” to proceed.

5. | Say the name of your phone whenprompted. - Use any name to uniquely describeyour phone.

6. | Bluetooth® system will repeat thename you stated.

7. | Say "Yes" to confirm.

The system may not function in the following cases:
If 5 phones have already been registered. If the system cannot communicate with the phone.

Connecting phone

When the Bluetooth® system is enabled,the phone previously used is automaticallyselected and re-connected. If youwant to select a different phone previouslypaired, the phone can be selectedthrough “Select Phone” menu.Only a selected phone can be used withthe hands-free system.

1. | Press button.

2. | Say "Set Up".

3. | Say "Select Phone" after prompt. - The system lists all the registeredphone names.

4. | Say the name or number of desiredphone from the list.

5. | Say "Yes" to confirm.

6. | By manual operation: - Select “SELECT” in PHONE menu,then select desired phone from thelist.

The system may not function in the following cases:
If the phone is not found.
If the system does not recognize the voice command.

Deleting phone

The paired phone can be deleted.

- | When the phone is deleted, all the informationassociated with that phone is also be deleted (including phonebook).

- | If you want to use the deleted phonewith the audio system again, pairingprocedure must be completed oncemore.

1. | Press button.

2. | Say "Set Up".

3. | Say “Delete Phone” after prompt. - The system lists all the registeredphone names.

4. | Say the name or number of desiredphone from the list.

5. | Say “Yes” to confirm.

6. | By manual operation: - Select “DELETE” in PHONE menu,then select desired phone from the list.

Changing Priority
When several phones are paired to theaudio system, the system attempts toconnect following order when theBluetooth® system is enabled:
1) “Priority” checked phone.
2) Previously connected phone.
3) Gives up auto connection.

1. | Press button.

2. | Say “Set Up”.

3. | Say “Change Priority” after prompt. - The system lists all the registeredphone names.

4. | Say the name or number of desiredphone from the list.

5. | Say “Yes” to confirm.

6. | By manual operation: - Select “PRIORITY” in PHONE menu,then select desired phone from thelist.

Bluetooth AVN System

• | Bluetooth allows wireless transmission of information between PC, mobile phones, headsets, PDAs, printers and other devices within close ranges by using 2.45Ghz frequency short-distance wireless telecommunication technologies."

• | Within this vehicle, users can make handsfree calls, transmit mobile phonedata, and play audio streaming files by connecting a mobile phone with the system.Functions supported by Functions supported by"

• | Pairing mobile phones. (Up to 5 phones)

• | Connecting/disconnecting mobile phones.

• | Making/Answering phone calls.

• | Downloading a Phone Book.

• | Downloading a Call history list.

• | Playing music saved in a Bluetooth phone in the vehicleSome functions may not be supported insome mobile phone.

in the vehicle
Some functions may not be supported in some mobile phone.