| SONATA(YF) >2013 > G 2.4 GDI > Steering System > Steering wheel>Repair procedures |

Replacement

1. | Disconnect the battery negative cable from the battery and then wait for at least 30 seconds.

2. | Turn the steering wheel so that the front wheels can face straight ahead.

3. | Remove the airbag module. (Refer to Restraint - "Driver Airbag (DAB) Module and Clock Spring")

4. | Disconnect the connector & lock nut (A) and then remove the steering wheel.