| SONATA(YF) >2013 > G 2.4 GDI > Steering System > Steering wheel > Flex Steer>Description and Operation |

Instruction

Flex Steer is system to choose the three modes power steering depending on driver preference or driving conditions.

• | Display on the cluster but power steering is would not changed while operating the steering wheel.

As a safety measures, mode is changed automatically when steering wheel operation is done.

• | Be sure to carefully change the mode while driving.

• | Electric Power Steering (MDPS) is not working due to the failure, "flex steer" is may not work.

How to operate

• | First input : Display the current mode on cluster. (4 seconds)

• | Add input (4 seconds) : Mode is changed sequentially.

• | Three steering modes

COMRORT : For the elder and the female drivers: it is mainly used for city driving and stop & parking, and a little lighter power steering.
NORMAL : Basic mode
SPORT : It is mainly used for highway driving, and a little heavy power steering.